ReadMe.txt for the Nordic Semiconductor nRF52832 start project.

This project was built for SEGGER Embedded Studio V5.20a.

Supported hardware:
===================
The sample project for the nRF52832 is prepared to run on
a Nordic Semiconductor nRF52 (Preview) Development Kit. Using
different target hardware may require modifications.

Configurations:
===============
- Debug:
  This configuration is prepared for download into internal
  Flash using J-Link. An embOS debug and profiling library
  is used.
  To use SEGGER SystemView with this configuration, configure
  SystemViewer for NRF52832_XXAA as target device and SWD at
  1000 kHz as target interface.

- Release:
  This configuration is prepared for download into internal
  Flash using J-Link. An embOS release library is used.
